- Processing
- p5.js
- Processing.py
- Processing for Android
- Processing for Pi

- Processing Foundation

This reference is for Processing 3.0+. If you have a previous version, use the reference included with your software in the Help menu. If you see any errors or have suggestions, please let us know. If you prefer a more technical reference, visit the Processing Core Javadoc and Libraries Javadoc.

Name | ### Capture
Examples |
    import processing.video.*;

    Capture cam;

    void setup() {
      size(640, 480);

      String[] cameras = Capture.list();

      if (cameras.length == 0) {
        println("There are no cameras available for capture.");
        exit();
      } else {
        println("Available cameras:");
        for (int i = 0; i < cameras.length; i++) {
          println(cameras[i]);
        }

        // The camera can be initialized directly using an
        // element from the array returned by list():
        cam = new Capture(this, cameras[0]);
        cam.start();
      }
    }

    void draw() {
      if (cam.available() == true) {
        cam.read();
      }
      image(cam, 0, 0);
      // The following does the same, and is faster when just drawing the image
      // without any additional resizing, transformations, or tint.
      //set(0, 0, cam);
    }
Description | Datatype for storing and manipulating video frames from an attached capture device such as a camera. Use Capture.list() to show the names of any attached devices. Using the version of the constructor without name will attempt to use the last device used by a QuickTime program.
Methods |
available() | Returns "true" when a new video frame is available to read
start() | Starts capturing frames from the selected device
stop() | Stops capturing frames from an attached device
read() | Reads the current video frame
list() | Gets a list of all available capture devices such as a camera
Constructor |
    Capture(parent)
    Capture(parent, requestConfig)
    Capture(parent, requestWidth, requestHeight)
    Capture(parent, requestWidth, requestHeight, frameRate)
    Capture(parent, requestWidth, requestHeight, cameraName)
    Capture(parent, requestWidth, requestHeight, cameraName, frameRate)
Parameters |
parent | PApplet: typically use "this"
requestWidth | int: width of the frame
requestHeight | int: height of the frame
frameRate | int: number of frames to read per second
cameraName | String: name of the camera

Updated on July 4, 2018 11:56:47am EDT