- Processing
- p5.js
- Processing.py
- Processing for Android
- Processing for Pi

- Processing Foundation

This reference is for Processing 3.0+. If you have a previous version, use the reference included with your software in the Help menu. If you see any errors or have suggestions, please let us know. If you prefer a more technical reference, visit the Processing Core Javadoc and Libraries Javadoc.

Class | Serial
Name | ### bufferUntil()
Examples |
    import processing.serial.*;

    Serial myPort;    // The serial port
    String inString;  // Input string from serial port
    int lf = 10;      // ASCII linefeed

    void setup() {
      size(400,200);
      // List all the available serial ports:
      printArray(Serial.list());
      // Open the port you are using at the rate you want:
      myPort = new Serial(this, Serial.list()[0], 9600);
      myPort.bufferUntil(lf);
    }

    void draw() {
      background(0);
      text("received: " + inString, 10,50);
    }

    void serialEvent(Serial p) {
      inString = p.readString();
    }
Description | Sets a specific byte to buffer until before calling serialEvent().
Syntax |
    serial.bufferUntil(inByte)
Parameters |
serial | Serial: any variable of type Serial
inByte | int: the value to buffer until
Returns | void

Updated on July 4, 2018 11:56:46am EDT