- Processing
- p5.js
- Processing.py
- Processing for Android
- Processing for Pi

- Processing Foundation

This reference is for Processing 3.0+. If you have a previous version, use the reference included with your software in the Help menu. If you see any errors or have suggestions, please let us know. If you prefer a more technical reference, visit the Processing Core Javadoc and Libraries Javadoc.

Class | Serial
Name | ### lastChar()
Examples |
    // Example by Tom Igoe

    import processing.serial.*;

    Serial myPort;  // The serial port:

    void setup() {
      // List all the available serial ports:
      printArray(Serial.list());
      // Open the port you are using at the rate you want:
      myPort = new Serial(this, Serial.list()[0], 9600);
      myPort.write(45);
    }

    void draw() {
      while (myPort.available() > 0) {
        char lastIn = myPort.lastChar();
        println(lastIn);
      }
    }
Description | Returns the last byte received as a char or -1 if there is none available.
Syntax |
    serial.lastChar()
Parameters |
serial | Serial: any variable of type Serial
Returns | char

Updated on July 4, 2018 11:56:46am EDT